**Aggregate Industries UK Ltd**

**Tel: 01285 646884**

**H62 RECONSTRUCTED STONE SLATING**

**03 ROOF SLATING**

Aggregate Industries manufacture a range of Bradstone reconstructed stone slates in a

number of finishes, shades and sizes. Manufactured principally from naturally

occurring aggregates, ordinary Portland cement and colour pigments, they are

moulded from hand-dressed natural stone slates by means of a specifically developed

technique which reproduces the fine detail of the originals on the textured face. A

range of masters is used to avoid noticeable repetition of profiles.

All of our Bradstone roofing slates comply with BS EN 490: 1994 (Concrete Roofing Tiles

and Fittings - Product Specifications). Product testing is carried out in accordance

with BS EN 490: 1994 (Concrete Roofing Tiles and Fittings - Test methods).

Aggregate Industries will calculate the superficial roof area and quote for

delivery of the required Bradstone roofing slates and fittings to all parts of the UK on

a supply only basis. On receipt of a firm order, they will schedule the actual quantities

of slates and fittings required. A battening and coursing guide for the specific roof

will be supplied and this should be strictly adhered to.